trixbox quick install guide

install the ISO

Warning: installing this ISO will format your computer and erase your hard drive

Boot a machine with the ISO. We recommend at least a 500MHZ PIII with 256megs of RAM. If you install any Digium hardware into the system it will be configured during the install.

Press enter to start the install process.

Enter the root password twice this will be the password you use when logging into the Linux command line.

The system will eject your CD. Take it out of the drive. After two automatic reboot your system should be ready.

Configuration

Login into you new trixbox with the username: root and the password you selected during installation

When you log in the system will tell you what IP address it received from your DHCP server. You can give the system a permanent address now by typing netconfig.

If you reconfigured the IP address reboot the system now by typing reboot.

To continue configuration connect to your system with a web browser

Click on Switch next to User Mode this will open the Admin GUI. Login with user:maint pass:password

Click on Asterisk -> FreePBX. This will open the FreePBX configuration GUI

Click on tools -> module admin. This will give you a list of modules you can install. Install the modules you want.

Click setup -> extensions -> sip and add your first extension.

Enter at least and extension number (200 is a good starting point) and a secret (abc123 is good). You should also enable voicemail for this extension. When you are done click the red commit bar at the top of the screen.

You have a PBX now you need a phone

You could use a VOIP phone, or an ATA to connect a normal analog phone to you trixbox but if you don’t have one of these install a soft phone on your Windows desktop computer.

One of the easiest to setup is X-lite. Plus its VERY NAT friendly! (sends out tiny NAT keepalives every 10 seconds to the server)

If X-Lite cannot connect, the setup screen should open, if not, click on the "drop down" icon just to the left of the green Off-Hook icon.

Under System Settings, select the SIP Proxy settings then double-click on the first entry. You will see the SIP Proxy settings as shown here. The settings I changed are as follows:

Username: 200 (my extension)
Authorization User: 200 (my extension again)
Password: abc123 (my extension password)
Domain Realm: 192.168.5.50 (trixbox IP address )
SIP Proxy: 192.168.5.50 (trixbox IP address )